{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Product Info","Technical Data","64-110 kV"],"read":"whole","date_system":"1900"}

{"sheet":"Product Info","index":0,"n_rows":4,"n_cols":2,"rows_kept":4}
["Product Name","N2X(F)K2Y"]
["SKU","N2X(F)K2Y-high-voltage-cables"]
["Category","Hochspannungskabel"]
["Description","The N2X(F)K2Y high-voltage cable series, designed for 64/110kV applications, utilizes copper conductors and XLPE insulation to meet the rigorous demands of industrial power distribution and transmission. These cables are engineered for high ampacity and fault current withstand in diverse installation environments."]

{"sheet":"Technical Data","index":1,"n_rows":2,"n_cols":2,"rows_kept":2}
["Property","Value"]
["Rated voltage (kV) [kV]","64/110"]

{"sheet":"64-110 kV","index":2,"n_rows":17,"n_cols":7,"rows_kept":17}
["Configuration/Cross-section","Cond.","RI [Ohm/km]","Wi [mm]","Rbv [mm]","Ø [mm]","G [kg/km]"]
["1×150RM","Cu","0.16","18","1.4","67","8300"]
["1×185RM","Cu","0.13","17","1.3","66","8400"]
["1×240RM","Cu","0.1","16.5","1.4","67","9030"]
["1×300RM","Cu","0.08","15.5","1.4","67","9540"]
["1×400RM","Cu","0.06","14.5","1.4","69","10410"]
["1×500RM","Cu","0.05","14","1.4","71","11590"]
["1×630RM","Cu","0.04","14","1.5","75","13470"]
["1×800RM","Cu","0.03","14","1.6","80","15590"]
["1×1000RM","Cu","0.03","14","1.7","84","17980"]
["1×1200RMS","Cu","0.02","14","1.8","89","20530"]
["1×1400RMS","Cu","0.02","14","1.9","94","22780"]
["1×1600RMS","Cu","0.02","14","2","98","25280"]
["1×1800RMS","Cu","0.02","14","2","102","27940"]
["1×2000RMS","Cu","0.02","14","2.1","103","29610"]
["1×2500RMS","Cu","0.01","14.5","2.2","112","35400"]
["1×3000RMS","Cu","0.01","14.5","2.4","121","42420"]